|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  | | --- | | **RECORD OF VISUAL HATCH COVER SURVEY** | | | | | | | | | |
|  | | | | | | | | |
|
|
|
|
|
|
|  | | | | | | | | |
|  | | | | | | | | |
|  | | | | | | | | |
|  | | | | | | | | |
| All correspondence should be addressed to the Managers | | | | | | | | |
|  |  |  |  |  |  |  |  |  |
|  |  | Name of ship | |  |  |  |  |  |
|  |  | Operator |  |  |  |  |  |  |
|  |  | Type of ship | |  |  |  |  |  |
|  |  | Year and country of build | | |  |  |  |  |
|  |  | Flag |  |  |  |  |  |  |
|  |  | Gross tonnage | |  |  |  |  |  |
|  |  | Classification Society | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  | Date(s) and place(s) of survey | | | Date | | Place | |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  | Name of Survey Company | | |  |  |  |  |  |
|  | Name of Surveyor | |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **ABC** |  |  | **NOT** | **NOT** | **YES** | **NO** |
| **No.** |  |  | **CHECKED** | **RELEVANT** |  |  |
| S1 | Can ship's staff confirm if the holds have been sea water washed? | |  |  |  |  |
| S2 | Can ship's staff confirm if the holds have been fresh water rinsed? | |  |  |  |  |
| S3 | Was the ship's certification relating to hatch cover weathertightness (Class survey) valid? | |  |  |  |  |
|  | [e.g. LR require this annually under | |  |  |  |  |
|  | Rule: Part 1, Chapter 3, Section 2.2.2(a)] | |  |  |  |  |
| 46 | Are external vents, sounding pipes and their closing appliances in good condition and correctly labelled? | |  |  |  |  |
|  |  | |  |  |  |  |
| 47 | Are all external watertight closures of deck openings in satisfactory condition and well maintained? | |  |  |  |  |
|  | (e.g. Access hatches) | |  |  |  |  |
| 59 | Are these items in | hatch cover panels / pontoons |  |  |  |  |
| 60 | satisfactory condition? | hinge pins, locators, wheels & axles |  |  |  |  |
| 61 |  | hatch cover seal packing or tarpaulins |  |  |  |  |
| 62 |  | seal packing channels |  |  |  |  |
| 63 |  | all cleats, wedges and securing bars |  |  |  |  |
| 64 |  | compression bars |  |  |  |  |
| 65 |  | coamings |  |  |  |  |
| 66 |  | drains and non-return arrangements |  |  |  |  |
| 67 |  | coaming tops and trackways |  |  |  |  |
| 68 | Are hatch covers free from the use of additional sealing methods? | |  |  |  |  |
|  | (e.g. sealing tape, expanding foam, cement and non-class approved systems) | |  |  |  |  |
| 69 | Are hatch coaming internal surfaces free of recent leakage | |  |  |  |  |
|  | indications? |  |  |  |  |  |
| 70 | Do hatch cover operating systems appear in satisfactory | |  |  |  |  |
|  | condition? |  |  |  |  |  |
| 140 | Can ship's staff confirm that records of regular testing of bilge systems are kept; including alarms? | |  |  |  |  |
|  |  | |  |  |  |  |
| 141 | Can ship's staff confirm that bilge soundings are logged daily? | |  |  |  |  |